;
; Copyright (c) SOFTARTS CO.,LTD. All rights reserved.
;
[Version]
Signature="$Windows NT$"
Class=Ports
ClassGUID={4d36e978-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
DriverVer=12/05/2011,2.0.0.11

[Manufacturer]
%Provider%=SECTION_0

[SECTION_0]
%DisplayName1002%=ComPort1002,savrcom\1002
%DisplayName1003%=ComPort1003,savrcom\1003
%DisplayName1004%=ComPort1004,savrcom\1004
%DisplayName1005%=ComPort1005,savrcom\1005

; ---- com7 ----
[ComPort1002.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort1002.NT.AddReg

[ComPort1002.NT.HW]
AddReg=ComPort.NT.HW.AddReg, ComPort1002.NT.HW.AddReg

[ComPort1002.NT.HW.AddReg]
HKR,,"TargetDevice",0x00010000,"VID_1008&PID_1002"

[ComPort1002.NT.Services]
AddService = savrcom, 0x00000002, Serial_Service_Inst

; ---- com8 ----
[ComPort1003.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort1003.NT.AddReg

[ComPort1003.NT.HW]
AddReg=ComPort.NT.HW.AddReg, ComPort1003.NT.HW.AddReg

[ComPort1003.NT.HW.AddReg]
HKR,,"TargetDevice",0x00010000,"VID_1008&PID_1003"

[ComPort1003.NT.Services]
AddService = savrcom, 0x00000002, Serial_Service_Inst

; ---- com9 ----
[ComPort1004.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort1004.NT.AddReg

[ComPort1004.NT.HW]
AddReg=ComPort.NT.HW.AddReg, ComPort1004.NT.HW.AddReg

[ComPort1004.NT.HW.AddReg]
HKR,,"TargetDevice",0x00010000,"VID_1008&PID_1004"

[ComPort1004.NT.Services]
AddService = savrcom, 0x00000002, Serial_Service_Inst

; ---- com10 ----
[ComPort1005.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort1005.NT.AddReg

[ComPort1005.NT.HW]
AddReg=ComPort.NT.HW.AddReg, ComPort1005.NT.HW.AddReg

[ComPort1005.NT.HW.AddReg]
HKR,,"TargetDevice",0x00010000,"VID_1008&PID_1005"

[ComPort1005.NT.Services]
AddService = savrcom, 0x00000002, Serial_Service_Inst

; ---- common ----
[ComPort.NT.Copy]
savrcom.sys

[ComPort.AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.NT.HW.AddReg]
HKR,,"EndPointCaps",0x00010001,3
HKR,,"DebugLevel",0x00010001,0x803
HKR,,"CxPollPeriod",0x00010001,0xffffffff
HKR,,"TxKickThreshold",0x00010001,256

[Serial_Service_Inst]
DisplayName    = %savrcom.SvcDesc%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 1               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\savrcom.sys
LoadOrderGroup = Extended base

[DestinationDirs]
DefaultDestDir=12

[SourceDisksFiles]
savrcom.sys=1

[SourceDisksNames]
1=%InstallDiskName%

[Strings]
Provider="SOFTARTS CO.,LTD"
DisplayName1002="Fujitsu Line Display VFD Kanji1"
DisplayName1003="Fujitsu Line Display VFD Kanji2"
DisplayName1004="Fujitsu Line Display VFD ANK1"
DisplayName1005="Fujitsu Line Display VFD ANK2"
InstallDiskName="savrcom Virtual Communication Port Setup Disk"
savrcom.SvcDesc="savrcom Virtual Communication Port"
