;******************************************************************************
;*
;*                           Hilscher GmbH
;*
;*                netX Driver Setup Information File
;*             for netX 500/100/10/51/52/4000 USB Bootmonitor 
;*  
;*  Variant for Bootwizard: 
;*  The device interface GUID is not set. This prevents the interface from being
;*  recognized by the plugin on composite devices, i.e. on netX 51/52, only the
;*  virtual COM port is listed.
;* 
;*******************************************************************************
;* File name: netx_usb_bootmonitor.inf
;*******************************************************************************
;*
;* Binds the following USB IDs to the WinUSB driver:
;* 
;*   VID   PID    REV   MI
;* 0x0cc4 0x0815 0x0100     netX500 Bootmonitor (ROM code)  
;* 0x1939 0x0015 0x0001     netX500 Bootmonitor (Soft)
;* 0x1939 0x000c 0x0001     netX10  Bootmonitor (ROM code)
;* 0x1939 0x000c 0x0002     netX10  Bootmonitor (Soft)
;* 0x1939 0x0018 0x0001 01  netX51  Bootmonitor (ROM code)
;* 0x1939 0x0018 0x0002 01  netX51  Bootmonitor (Soft)
;* 0x1939 0x0019 0x0001 01  netX52  Bootmonitor (ROM code)
;* 0x1939 0x0019 0x0002 01  netX52  Bootmonitor (Soft)
;* 0x1939 0x0020 0x0001 01  netX4000 Relaxed Bootmonitor 
;* 0x1939 0x002a 0x0002 01  netX4000 Full    Bootmonitor 
;* 0x1939 0x002b 0x0002 01  netX4100 Small   Bootmonitor 
;* 
;*******************************************************************************
; Copyright (c) 2010 libusb (GNU LGPL)


[Version]
Signature   = "$Windows NT$"
Class       = "Universal Serial Bus devices"
ClassGuid   = {88bae032-5a81-49f0-bc3d-a4ff138216d6}
Provider    = "Hilscher GmbH"
CatalogFile = netx_usb_bootmonitor.cat
DriverVer   = 10/16/2018,2.4.7
DriverPackageDisplayName = "USB driver for the netX10/51/52/100/500/4000 ROM code"

[Strings]
VendorName = "Hilscher Gesellschaft für Systemautomation mbH"
SourceName = "netX USB Bootmonitor Install Disk"

DeviceName_netX500ROM       = "netX500 USB Bootmonitor (ROM)"
DeviceID_netX500ROM         = "VID_0CC4&PID_0815&REV_0100"
                            
DeviceName_netX500Soft      = "netX500 USB Bootmonitor (V2)"
DeviceID_netX500Soft        = "VID_1939&PID_0015&REV_0001"
                            
DeviceName_netX10ROM        = "netX10 USB Bootmonitor (ROM)"
DeviceID_netX10ROM          = "VID_1939&PID_000C&REV_0001"
                            
DeviceName_netX10Soft       = "netX10 USB Bootmonitor (V2)"
DeviceID_netX10Soft         = "VID_1939&PID_000C&REV_0002"
                            
DeviceName_netX51ROM        = "netX51 USB Bootmonitor (ROM)"
DeviceID_netX51ROM          = "VID_1939&PID_0018&REV_0001&MI_01"
                            
DeviceName_netX51Soft       = "netX51 USB Bootmonitor (V2)"
DeviceID_netX51Soft         = "VID_1939&PID_0018&REV_0002&MI_01"
                            
DeviceName_netX52ROM        = "netX52 USB Bootmonitor (ROM)"
DeviceID_netX52ROM          = "VID_1939&PID_0019&REV_0001&MI_01"
                            
DeviceName_netX52Soft       = "netX52 USB Bootmonitor (V2)"
DeviceID_netX52Soft         = "VID_1939&PID_0019&REV_0002&MI_01"

DeviceName_netX4000RlxdROM  = "netX4000 Relaxed USB Bootmonitor"
DeviceID_netX4000RlxdROM    = "VID_1939&PID_0020&REV_0001&MI_01"

DeviceName_netX4000FullROM  = "netX4000 Full USB Bootmonitor"
DeviceID_netX4000FullROM    = "VID_1939&PID_002a&REV_0002&MI_01"

DeviceName_netX4100SmallROM = "netX4100 Small USB Bootmonitor"
DeviceID_netX4100SmallROM   = "VID_1939&PID_002b&REV_0002&MI_01"


[ClassInstall32]
Addreg = WinUSBDeviceClassReg

[WinUSBDeviceClassReg]
HKR,,,0,"Universal Serial Bus devices"
HKR,,Icon,,-20

[Manufacturer]
%VendorName% = libusbDevice_WinUSB,NTx86,NTamd64,NTia64

[libusbDevice_WinUSB.NTx86]
%DeviceName_netX500ROM%        = USB_Install, USB\%DeviceID_netX500ROM%
%DeviceName_netX500Soft%       = USB_Install, USB\%DeviceID_netX500Soft%
%DeviceName_netX10ROM%         = USB_Install, USB\%DeviceID_netX10ROM%
%DeviceName_netX10Soft%        = USB_Install, USB\%DeviceID_netX10Soft%
%DeviceName_netX51ROM%         = USB_Install, USB\%DeviceID_netX51ROM%
%DeviceName_netX51Soft%        = USB_Install, USB\%DeviceID_netX51Soft%
%DeviceName_netX52ROM%         = USB_Install, USB\%DeviceID_netX52ROM%
%DeviceName_netX52Soft%        = USB_Install, USB\%DeviceID_netX52Soft%
%DeviceName_netX4000RlxdROM%   = USB_Install, USB\%DeviceID_netX4000RlxdROM%
%DeviceName_netX4000FullROM%   = USB_Install, USB\%DeviceID_netX4000FullROM%
%DeviceName_netX4100SmallROM%  = USB_Install, USB\%DeviceID_netX4100SmallROM%

[libusbDevice_WinUSB.NTamd64]
%DeviceName_netX500ROM%        = USB_Install, USB\%DeviceID_netX500ROM%
%DeviceName_netX500Soft%       = USB_Install, USB\%DeviceID_netX500Soft%
%DeviceName_netX10ROM%         = USB_Install, USB\%DeviceID_netX10ROM%
%DeviceName_netX10Soft%        = USB_Install, USB\%DeviceID_netX10Soft%
%DeviceName_netX51ROM%         = USB_Install, USB\%DeviceID_netX51ROM%
%DeviceName_netX51Soft%        = USB_Install, USB\%DeviceID_netX51Soft%
%DeviceName_netX52ROM%         = USB_Install, USB\%DeviceID_netX52ROM%
%DeviceName_netX52Soft%        = USB_Install, USB\%DeviceID_netX52Soft%
%DeviceName_netX4000RlxdROM%   = USB_Install, USB\%DeviceID_netX4000RlxdROM%
%DeviceName_netX4000FullROM%   = USB_Install, USB\%DeviceID_netX4000FullROM%
%DeviceName_netX4100SmallROM%  = USB_Install, USB\%DeviceID_netX4100SmallROM%

[libusbDevice_WinUSB.NTia64]
%DeviceName_netX500ROM%        = USB_Install, USB\%DeviceID_netX500ROM%
%DeviceName_netX500Soft%       = USB_Install, USB\%DeviceID_netX500Soft%
%DeviceName_netX10ROM%         = USB_Install, USB\%DeviceID_netX10ROM%
%DeviceName_netX10Soft%        = USB_Install, USB\%DeviceID_netX10Soft%
%DeviceName_netX51ROM%         = USB_Install, USB\%DeviceID_netX51ROM%
%DeviceName_netX51Soft%        = USB_Install, USB\%DeviceID_netX51Soft%
%DeviceName_netX52ROM%         = USB_Install, USB\%DeviceID_netX52ROM%
%DeviceName_netX52Soft%        = USB_Install, USB\%DeviceID_netX52Soft%
%DeviceName_netX4000RlxdROM%   = USB_Install, USB\%DeviceID_netX4000RlxdROM%
%DeviceName_netX4000FullROM%   = USB_Install, USB\%DeviceID_netX4000FullROM%
%DeviceName_netX4100SmallROM%  = USB_Install, USB\%DeviceID_netX4100SmallROM%


[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include    = winusb.inf
AddService = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName   = "WinUSB - Kernel Driver 07/14/2009 6.1.7600.16385"
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUsb_Install

[WinUSB_Install]
KmdfLibraryVersion = 1.9

[USB_Install.HW]
AddReg = NoDeviceInterfaceGUID

[NoDeviceInterfaceGUID]
; Avoids adding a DeviceInterfaceGUID for generic driver

[AddDeviceInterfaceGUID]
HKR,,DeviceInterfaceGUIDs,0x10000,%DeviceGUID%

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles = 11

[SourceDisksNames]
1 = %SourceName%

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1,x86
WdfCoInstaller01009.dll = 1,x86

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 1,amd64
WdfCoInstaller01009.dll = 1,amd64

[SourceDisksFiles.ia64]
WinUSBCoInstaller2.dll  = 1,ia64
WdfCoInstaller01009.dll = 1,ia64
