; ======== libusb 1.0 (WinUSB) device driver ==========

; ===================== Strings =======================

[Strings]

DeviceGUID = "{ffe1ce84-18a1-4cf9-ac16-df74b7958daa}"
DeviceClassGUID = "{78a1c341-4539-11d3-b88d-00c04fad5171}"

ProviderName = "libusb 1.0"
WinUSB_SvcDesc = "WinUSB Driver Service"
DiskName = "libusb (WinUSB) Device Install Disk"
ClassName = "libusb (WinUSB) devices"

; ====================== Version ======================

[Version]
DriverVer = 08/22/2018,1.0.22.11315
Signature = "$Windows NT$"
Class = %ClassName%
ClassGuid = %DeviceClassGUID%
Provider = %ProviderName%
CatalogFile = libusb_device.cat

; =================== Class section ===================

; Since the device is not a standard USB device, we define a new class for it.
[ClassInstall32]
Addreg = WinUSBDeviceClassReg

[WinUSBDeviceClassReg]
HKR,,,0,%ClassName%
; -20 is for the USB icon
HKR,,Icon,,-20

; =========== Manufacturer/Models sections ============

[Manufacturer]
%ProviderName% = libusbDevice_WinUSB,NTx86,NTamd64,NTarm64

[libusbDevice_WinUSB.NTx86]
; BEGIN_USB_DEVICES LibUSB-1.0

; Device: 0403:6001
; Generic Identifier
; Vendor: Future Technology Devices International, Ltd
; Product: FT232 USB-Serial (UART) IC
"LibUSB-1.0: Albatross [all models], Cebra [all models], HIMS [Sync Braille], HandyTech [FTDI chip], MDV [all models]"=LIBUSB_DEV, USB\VID_0403&PID_6001

; Device: 0403:DE58
"LibUSB-1.0: Hedo [MobilLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE58

; Device: 0403:DE59
"LibUSB-1.0: Hedo [ProfiLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE59

; Device: 0403:F208
"LibUSB-1.0: Papenmeier [all models]"=LIBUSB_DEV, USB\VID_0403&PID_F208

; Device: 0403:FE70
"LibUSB-1.0: Baum [Vario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE70

; Device: 0403:FE71
"LibUSB-1.0: Baum [PocketVario (24 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE71

; Device: 0403:FE72
"LibUSB-1.0: Baum [SuperVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE72

; Device: 0403:FE73
"LibUSB-1.0: Baum [SuperVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE73

; Device: 0403:FE74
"LibUSB-1.0: Baum [SuperVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE74

; Device: 0403:FE75
"LibUSB-1.0: Baum [SuperVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE75

; Device: 0403:FE76
"LibUSB-1.0: Baum [VarioPro 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE76

; Device: 0403:FE77
"LibUSB-1.0: Baum [VarioPro 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE77

; Device: 0452:0100
"LibUSB-1.0: Metec [all models]"=LIBUSB_DEV, USB\VID_0452&PID_0100

; Device: 045E:930A
"LibUSB-1.0: HIMS [Braille Sense (USB 1.1)], HIMS [Braille Sense (USB 2.0)], HIMS [Braille Sense U2 (USB 2.0)]"=LIBUSB_DEV, USB\VID_045E&PID_930A

; Device: 045E:930B
"LibUSB-1.0: HIMS [Braille Edge]"=LIBUSB_DEV, USB\VID_045E&PID_930B

; Device: 0483:A1D3
"LibUSB-1.0: Baum [Orbit 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0483&PID_A1D3

; Device: 06B0:0001
"LibUSB-1.0: Alva [Satellite (5nn)]"=LIBUSB_DEV, USB\VID_06B0&PID_0001

; Device: 0798:0001
"LibUSB-1.0: Voyager [all models]"=LIBUSB_DEV, USB\VID_0798&PID_0001

; Device: 0798:0600
"LibUSB-1.0: Alva [Voyager Protocol Converter]"=LIBUSB_DEV, USB\VID_0798&PID_0600

; Device: 0798:0624
"LibUSB-1.0: Alva [BC624]"=LIBUSB_DEV, USB\VID_0798&PID_0624

; Device: 0798:0640
"LibUSB-1.0: Alva [BC640]"=LIBUSB_DEV, USB\VID_0798&PID_0640

; Device: 0798:0680
"LibUSB-1.0: Alva [BC680]"=LIBUSB_DEV, USB\VID_0798&PID_0680

; Device: 0904:2000
"LibUSB-1.0: Baum [VarioPro 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2000

; Device: 0904:2001
"LibUSB-1.0: Baum [EcoVario 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2001

; Device: 0904:2002
"LibUSB-1.0: Baum [EcoVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2002

; Device: 0904:2007
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2007

; Device: 0904:2008
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2008

; Device: 0904:2009
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2009

; Device: 0904:2010
"LibUSB-1.0: Baum [VarioConnect 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2010

; Device: 0904:2011
"LibUSB-1.0: Baum [VarioConnect 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2011

; Device: 0904:2014
"LibUSB-1.0: Baum [EcoVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2014

; Device: 0904:2015
"LibUSB-1.0: Baum [EcoVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2015

; Device: 0904:2016
"LibUSB-1.0: Baum [EcoVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2016

; Device: 0904:3000
"LibUSB-1.0: Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3000

; Device: 0904:3001
"LibUSB-1.0: Baum [Orbit in Refreshabraille Emulation Mode (18 cells)], Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3001

; Device: 0904:4004
"LibUSB-1.0: Baum [Pronto! V3 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4004

; Device: 0904:4005
"LibUSB-1.0: Baum [Pronto! V3 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4005

; Device: 0904:4007
"LibUSB-1.0: Baum [Pronto! V4 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4007

; Device: 0904:4008
"LibUSB-1.0: Baum [Pronto! V4 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4008

; Device: 0904:6001
"LibUSB-1.0: Baum [SuperVario2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6001

; Device: 0904:6002
"LibUSB-1.0: Baum [PocketVario2 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6002

; Device: 0904:6003
"LibUSB-1.0: Baum [SuperVario2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6003

; Device: 0904:6004
"LibUSB-1.0: Baum [SuperVario2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6004

; Device: 0904:6005
"LibUSB-1.0: Baum [SuperVario2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6005

; Device: 0904:6006
"LibUSB-1.0: Baum [Brailliant2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6006

; Device: 0904:6007
"LibUSB-1.0: Baum [Brailliant2 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6007

; Device: 0904:6008
"LibUSB-1.0: Baum [Brailliant2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6008

; Device: 0904:6009
"LibUSB-1.0: Baum [Brailliant2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6009

; Device: 0904:600A
"LibUSB-1.0: Baum [Brailliant2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_600A

; Device: 0904:6011
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6011

; Device: 0904:6012
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6012

; Device: 0904:6013
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6013

; Device: 0904:6101
"LibUSB-1.0: Baum [VarioUltra 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6101

; Device: 0904:6102
"LibUSB-1.0: Baum [VarioUltra 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6102

; Device: 0904:6103
"LibUSB-1.0: Baum [VarioUltra 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6103

; Device: 0921:1200
"LibUSB-1.0: HandyTech [GoHubs chip]"=LIBUSB_DEV, USB\VID_0921&PID_1200

; Device: 0F4E:0100
"LibUSB-1.0: FreedomScientific [Focus 1]"=LIBUSB_DEV, USB\VID_0F4E&PID_0100

; Device: 0F4E:0111
"LibUSB-1.0: FreedomScientific [PAC Mate]"=LIBUSB_DEV, USB\VID_0F4E&PID_0111

; Device: 0F4E:0112
"LibUSB-1.0: FreedomScientific [Focus 2]"=LIBUSB_DEV, USB\VID_0F4E&PID_0112

; Device: 0F4E:0114
"LibUSB-1.0: FreedomScientific [Focus Blue]"=LIBUSB_DEV, USB\VID_0F4E&PID_0114

; Device: 10C4:EA60
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge / myAVR mySmartUSB light
"LibUSB-1.0: BrailleMemo [Pocket], Seika [Braille Display]"=LIBUSB_DEV, USB\VID_10C4&PID_EA60

; Device: 10C4:EA80
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge
"LibUSB-1.0: Seika [Note Taker]"=LIBUSB_DEV, USB\VID_10C4&PID_EA80

; Device: 1148:0301
"LibUSB-1.0: BrailleMemo [Smart]"=LIBUSB_DEV, USB\VID_1148&PID_0301

; Device: 1209:ABC0
"LibUSB-1.0: Inceptor [all models]"=LIBUSB_DEV, USB\VID_1209&PID_ABC0

; Device: 1C71:C004
"LibUSB-1.0: BrailleNote [HumanWare APEX]"=LIBUSB_DEV, USB\VID_1C71&PID_C004

; Device: 1C71:C005
"LibUSB-1.0: HumanWare [all models (serial protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C005

; Device: 1C71:C006
"LibUSB-1.0: HumanWare [non-Touch models (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C006

; Device: 1C71:C00A
"LibUSB-1.0: HumanWare [BrailleNote Touch (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C00A

; Device: 1FE4:0003
"LibUSB-1.0: HandyTech [USB-HID adapter]"=LIBUSB_DEV, USB\VID_1FE4&PID_0003

; Device: 1FE4:0044
"LibUSB-1.0: HandyTech [Easy Braille (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0044

; Device: 1FE4:0054
"LibUSB-1.0: HandyTech [Active Braille]"=LIBUSB_DEV, USB\VID_1FE4&PID_0054

; Device: 1FE4:0055
"LibUSB-1.0: HandyTech [Connect Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0055

; Device: 1FE4:0061
"LibUSB-1.0: HandyTech [Actilino]"=LIBUSB_DEV, USB\VID_1FE4&PID_0061

; Device: 1FE4:0064
"LibUSB-1.0: HandyTech [Active Star 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0064

; Device: 1FE4:0074
"LibUSB-1.0: HandyTech [Braille Star 40 (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0074

; Device: 1FE4:0081
"LibUSB-1.0: HandyTech [Basic Braille 16]"=LIBUSB_DEV, USB\VID_1FE4&PID_0081

; Device: 1FE4:0082
"LibUSB-1.0: HandyTech [Basic Braille 20]"=LIBUSB_DEV, USB\VID_1FE4&PID_0082

; Device: 1FE4:0083
"LibUSB-1.0: HandyTech [Basic Braille 32]"=LIBUSB_DEV, USB\VID_1FE4&PID_0083

; Device: 1FE4:0084
"LibUSB-1.0: HandyTech [Basic Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0084

; Device: 1FE4:0086
"LibUSB-1.0: HandyTech [Basic Braille 64]"=LIBUSB_DEV, USB\VID_1FE4&PID_0086

; Device: 1FE4:0087
"LibUSB-1.0: HandyTech [Basic Braille 80]"=LIBUSB_DEV, USB\VID_1FE4&PID_0087

; Device: 1FE4:008A
"LibUSB-1.0: HandyTech [Basic Braille 48]"=LIBUSB_DEV, USB\VID_1FE4&PID_008A

; Device: 1FE4:008B
"LibUSB-1.0: HandyTech [Basic Braille 160]"=LIBUSB_DEV, USB\VID_1FE4&PID_008B

; Device: 4242:0001
"LibUSB-1.0: Pegasus [all models]"=LIBUSB_DEV, USB\VID_4242&PID_0001

; Device: C251:1122
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1122

; Device: C251:1123
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1123

; Device: C251:1124
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1124

; Device: C251:1125
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1125

; Device: C251:1126
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1126

; Device: C251:1127
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1127

; Device: C251:1128
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1128

; Device: C251:1129
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1129

; Device: C251:112A
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112A

; Device: C251:112B
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112B

; Device: C251:112C
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112C

; Device: C251:112D
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112D

; Device: C251:112E
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112E

; Device: C251:112F
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112F

; Device: C251:1130
"LibUSB-1.0: EuroBraille [Esytime (firmware 1.03, 2014-03-31)], EuroBraille [Esytime]"=LIBUSB_DEV, USB\VID_C251&PID_1130

; Device: C251:1131
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1131

; Device: C251:1132
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1132

; END_USB_DEVICES

[libusbDevice_WinUSB.NTamd64]
; BEGIN_USB_DEVICES LibUSB-1.0

; Device: 0403:6001
; Generic Identifier
; Vendor: Future Technology Devices International, Ltd
; Product: FT232 USB-Serial (UART) IC
"LibUSB-1.0: Albatross [all models], Cebra [all models], HIMS [Sync Braille], HandyTech [FTDI chip], MDV [all models]"=LIBUSB_DEV, USB\VID_0403&PID_6001

; Device: 0403:DE58
"LibUSB-1.0: Hedo [MobilLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE58

; Device: 0403:DE59
"LibUSB-1.0: Hedo [ProfiLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE59

; Device: 0403:F208
"LibUSB-1.0: Papenmeier [all models]"=LIBUSB_DEV, USB\VID_0403&PID_F208

; Device: 0403:FE70
"LibUSB-1.0: Baum [Vario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE70

; Device: 0403:FE71
"LibUSB-1.0: Baum [PocketVario (24 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE71

; Device: 0403:FE72
"LibUSB-1.0: Baum [SuperVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE72

; Device: 0403:FE73
"LibUSB-1.0: Baum [SuperVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE73

; Device: 0403:FE74
"LibUSB-1.0: Baum [SuperVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE74

; Device: 0403:FE75
"LibUSB-1.0: Baum [SuperVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE75

; Device: 0403:FE76
"LibUSB-1.0: Baum [VarioPro 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE76

; Device: 0403:FE77
"LibUSB-1.0: Baum [VarioPro 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE77

; Device: 0452:0100
"LibUSB-1.0: Metec [all models]"=LIBUSB_DEV, USB\VID_0452&PID_0100

; Device: 045E:930A
"LibUSB-1.0: HIMS [Braille Sense (USB 1.1)], HIMS [Braille Sense (USB 2.0)], HIMS [Braille Sense U2 (USB 2.0)]"=LIBUSB_DEV, USB\VID_045E&PID_930A

; Device: 045E:930B
"LibUSB-1.0: HIMS [Braille Edge]"=LIBUSB_DEV, USB\VID_045E&PID_930B

; Device: 0483:A1D3
"LibUSB-1.0: Baum [Orbit 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0483&PID_A1D3

; Device: 06B0:0001
"LibUSB-1.0: Alva [Satellite (5nn)]"=LIBUSB_DEV, USB\VID_06B0&PID_0001

; Device: 0798:0001
"LibUSB-1.0: Voyager [all models]"=LIBUSB_DEV, USB\VID_0798&PID_0001

; Device: 0798:0600
"LibUSB-1.0: Alva [Voyager Protocol Converter]"=LIBUSB_DEV, USB\VID_0798&PID_0600

; Device: 0798:0624
"LibUSB-1.0: Alva [BC624]"=LIBUSB_DEV, USB\VID_0798&PID_0624

; Device: 0798:0640
"LibUSB-1.0: Alva [BC640]"=LIBUSB_DEV, USB\VID_0798&PID_0640

; Device: 0798:0680
"LibUSB-1.0: Alva [BC680]"=LIBUSB_DEV, USB\VID_0798&PID_0680

; Device: 0904:2000
"LibUSB-1.0: Baum [VarioPro 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2000

; Device: 0904:2001
"LibUSB-1.0: Baum [EcoVario 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2001

; Device: 0904:2002
"LibUSB-1.0: Baum [EcoVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2002

; Device: 0904:2007
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2007

; Device: 0904:2008
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2008

; Device: 0904:2009
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2009

; Device: 0904:2010
"LibUSB-1.0: Baum [VarioConnect 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2010

; Device: 0904:2011
"LibUSB-1.0: Baum [VarioConnect 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2011

; Device: 0904:2014
"LibUSB-1.0: Baum [EcoVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2014

; Device: 0904:2015
"LibUSB-1.0: Baum [EcoVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2015

; Device: 0904:2016
"LibUSB-1.0: Baum [EcoVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2016

; Device: 0904:3000
"LibUSB-1.0: Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3000

; Device: 0904:3001
"LibUSB-1.0: Baum [Orbit in Refreshabraille Emulation Mode (18 cells)], Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3001

; Device: 0904:4004
"LibUSB-1.0: Baum [Pronto! V3 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4004

; Device: 0904:4005
"LibUSB-1.0: Baum [Pronto! V3 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4005

; Device: 0904:4007
"LibUSB-1.0: Baum [Pronto! V4 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4007

; Device: 0904:4008
"LibUSB-1.0: Baum [Pronto! V4 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4008

; Device: 0904:6001
"LibUSB-1.0: Baum [SuperVario2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6001

; Device: 0904:6002
"LibUSB-1.0: Baum [PocketVario2 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6002

; Device: 0904:6003
"LibUSB-1.0: Baum [SuperVario2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6003

; Device: 0904:6004
"LibUSB-1.0: Baum [SuperVario2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6004

; Device: 0904:6005
"LibUSB-1.0: Baum [SuperVario2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6005

; Device: 0904:6006
"LibUSB-1.0: Baum [Brailliant2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6006

; Device: 0904:6007
"LibUSB-1.0: Baum [Brailliant2 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6007

; Device: 0904:6008
"LibUSB-1.0: Baum [Brailliant2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6008

; Device: 0904:6009
"LibUSB-1.0: Baum [Brailliant2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6009

; Device: 0904:600A
"LibUSB-1.0: Baum [Brailliant2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_600A

; Device: 0904:6011
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6011

; Device: 0904:6012
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6012

; Device: 0904:6013
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6013

; Device: 0904:6101
"LibUSB-1.0: Baum [VarioUltra 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6101

; Device: 0904:6102
"LibUSB-1.0: Baum [VarioUltra 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6102

; Device: 0904:6103
"LibUSB-1.0: Baum [VarioUltra 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6103

; Device: 0921:1200
"LibUSB-1.0: HandyTech [GoHubs chip]"=LIBUSB_DEV, USB\VID_0921&PID_1200

; Device: 0F4E:0100
"LibUSB-1.0: FreedomScientific [Focus 1]"=LIBUSB_DEV, USB\VID_0F4E&PID_0100

; Device: 0F4E:0111
"LibUSB-1.0: FreedomScientific [PAC Mate]"=LIBUSB_DEV, USB\VID_0F4E&PID_0111

; Device: 0F4E:0112
"LibUSB-1.0: FreedomScientific [Focus 2]"=LIBUSB_DEV, USB\VID_0F4E&PID_0112

; Device: 0F4E:0114
"LibUSB-1.0: FreedomScientific [Focus Blue]"=LIBUSB_DEV, USB\VID_0F4E&PID_0114

; Device: 10C4:EA60
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge / myAVR mySmartUSB light
"LibUSB-1.0: BrailleMemo [Pocket], Seika [Braille Display]"=LIBUSB_DEV, USB\VID_10C4&PID_EA60

; Device: 10C4:EA80
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge
"LibUSB-1.0: Seika [Note Taker]"=LIBUSB_DEV, USB\VID_10C4&PID_EA80

; Device: 1148:0301
"LibUSB-1.0: BrailleMemo [Smart]"=LIBUSB_DEV, USB\VID_1148&PID_0301

; Device: 1209:ABC0
"LibUSB-1.0: Inceptor [all models]"=LIBUSB_DEV, USB\VID_1209&PID_ABC0

; Device: 1C71:C004
"LibUSB-1.0: BrailleNote [HumanWare APEX]"=LIBUSB_DEV, USB\VID_1C71&PID_C004

; Device: 1C71:C005
"LibUSB-1.0: HumanWare [all models (serial protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C005

; Device: 1C71:C006
"LibUSB-1.0: HumanWare [non-Touch models (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C006

; Device: 1C71:C00A
"LibUSB-1.0: HumanWare [BrailleNote Touch (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C00A

; Device: 1FE4:0003
"LibUSB-1.0: HandyTech [USB-HID adapter]"=LIBUSB_DEV, USB\VID_1FE4&PID_0003

; Device: 1FE4:0044
"LibUSB-1.0: HandyTech [Easy Braille (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0044

; Device: 1FE4:0054
"LibUSB-1.0: HandyTech [Active Braille]"=LIBUSB_DEV, USB\VID_1FE4&PID_0054

; Device: 1FE4:0055
"LibUSB-1.0: HandyTech [Connect Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0055

; Device: 1FE4:0061
"LibUSB-1.0: HandyTech [Actilino]"=LIBUSB_DEV, USB\VID_1FE4&PID_0061

; Device: 1FE4:0064
"LibUSB-1.0: HandyTech [Active Star 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0064

; Device: 1FE4:0074
"LibUSB-1.0: HandyTech [Braille Star 40 (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0074

; Device: 1FE4:0081
"LibUSB-1.0: HandyTech [Basic Braille 16]"=LIBUSB_DEV, USB\VID_1FE4&PID_0081

; Device: 1FE4:0082
"LibUSB-1.0: HandyTech [Basic Braille 20]"=LIBUSB_DEV, USB\VID_1FE4&PID_0082

; Device: 1FE4:0083
"LibUSB-1.0: HandyTech [Basic Braille 32]"=LIBUSB_DEV, USB\VID_1FE4&PID_0083

; Device: 1FE4:0084
"LibUSB-1.0: HandyTech [Basic Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0084

; Device: 1FE4:0086
"LibUSB-1.0: HandyTech [Basic Braille 64]"=LIBUSB_DEV, USB\VID_1FE4&PID_0086

; Device: 1FE4:0087
"LibUSB-1.0: HandyTech [Basic Braille 80]"=LIBUSB_DEV, USB\VID_1FE4&PID_0087

; Device: 1FE4:008A
"LibUSB-1.0: HandyTech [Basic Braille 48]"=LIBUSB_DEV, USB\VID_1FE4&PID_008A

; Device: 1FE4:008B
"LibUSB-1.0: HandyTech [Basic Braille 160]"=LIBUSB_DEV, USB\VID_1FE4&PID_008B

; Device: 4242:0001
"LibUSB-1.0: Pegasus [all models]"=LIBUSB_DEV, USB\VID_4242&PID_0001

; Device: C251:1122
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1122

; Device: C251:1123
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1123

; Device: C251:1124
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1124

; Device: C251:1125
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1125

; Device: C251:1126
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1126

; Device: C251:1127
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1127

; Device: C251:1128
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1128

; Device: C251:1129
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1129

; Device: C251:112A
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112A

; Device: C251:112B
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112B

; Device: C251:112C
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112C

; Device: C251:112D
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112D

; Device: C251:112E
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112E

; Device: C251:112F
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112F

; Device: C251:1130
"LibUSB-1.0: EuroBraille [Esytime (firmware 1.03, 2014-03-31)], EuroBraille [Esytime]"=LIBUSB_DEV, USB\VID_C251&PID_1130

; Device: C251:1131
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1131

; Device: C251:1132
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1132

; END_USB_DEVICES

[libusbDevice_WinUSB.NTarm64]
; BEGIN_USB_DEVICES LibUSB-1.0

; Device: 0403:6001
; Generic Identifier
; Vendor: Future Technology Devices International, Ltd
; Product: FT232 USB-Serial (UART) IC
"LibUSB-1.0: Albatross [all models], Cebra [all models], HIMS [Sync Braille], HandyTech [FTDI chip], MDV [all models]"=LIBUSB_DEV, USB\VID_0403&PID_6001

; Device: 0403:DE58
"LibUSB-1.0: Hedo [MobilLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE58

; Device: 0403:DE59
"LibUSB-1.0: Hedo [ProfiLine]"=LIBUSB_DEV, USB\VID_0403&PID_DE59

; Device: 0403:F208
"LibUSB-1.0: Papenmeier [all models]"=LIBUSB_DEV, USB\VID_0403&PID_F208

; Device: 0403:FE70
"LibUSB-1.0: Baum [Vario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE70

; Device: 0403:FE71
"LibUSB-1.0: Baum [PocketVario (24 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE71

; Device: 0403:FE72
"LibUSB-1.0: Baum [SuperVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE72

; Device: 0403:FE73
"LibUSB-1.0: Baum [SuperVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE73

; Device: 0403:FE74
"LibUSB-1.0: Baum [SuperVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE74

; Device: 0403:FE75
"LibUSB-1.0: Baum [SuperVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE75

; Device: 0403:FE76
"LibUSB-1.0: Baum [VarioPro 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE76

; Device: 0403:FE77
"LibUSB-1.0: Baum [VarioPro 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0403&PID_FE77

; Device: 0452:0100
"LibUSB-1.0: Metec [all models]"=LIBUSB_DEV, USB\VID_0452&PID_0100

; Device: 045E:930A
"LibUSB-1.0: HIMS [Braille Sense (USB 1.1)], HIMS [Braille Sense (USB 2.0)], HIMS [Braille Sense U2 (USB 2.0)]"=LIBUSB_DEV, USB\VID_045E&PID_930A

; Device: 045E:930B
"LibUSB-1.0: HIMS [Braille Edge]"=LIBUSB_DEV, USB\VID_045E&PID_930B

; Device: 0483:A1D3
"LibUSB-1.0: Baum [Orbit 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0483&PID_A1D3

; Device: 06B0:0001
"LibUSB-1.0: Alva [Satellite (5nn)]"=LIBUSB_DEV, USB\VID_06B0&PID_0001

; Device: 0798:0001
"LibUSB-1.0: Voyager [all models]"=LIBUSB_DEV, USB\VID_0798&PID_0001

; Device: 0798:0600
"LibUSB-1.0: Alva [Voyager Protocol Converter]"=LIBUSB_DEV, USB\VID_0798&PID_0600

; Device: 0798:0624
"LibUSB-1.0: Alva [BC624]"=LIBUSB_DEV, USB\VID_0798&PID_0624

; Device: 0798:0640
"LibUSB-1.0: Alva [BC640]"=LIBUSB_DEV, USB\VID_0798&PID_0640

; Device: 0798:0680
"LibUSB-1.0: Alva [BC680]"=LIBUSB_DEV, USB\VID_0798&PID_0680

; Device: 0904:2000
"LibUSB-1.0: Baum [VarioPro 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2000

; Device: 0904:2001
"LibUSB-1.0: Baum [EcoVario 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2001

; Device: 0904:2002
"LibUSB-1.0: Baum [EcoVario 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2002

; Device: 0904:2007
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2007

; Device: 0904:2008
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2008

; Device: 0904:2009
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2009

; Device: 0904:2010
"LibUSB-1.0: Baum [VarioConnect 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2010

; Device: 0904:2011
"LibUSB-1.0: Baum [VarioConnect 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2011

; Device: 0904:2014
"LibUSB-1.0: Baum [EcoVario 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2014

; Device: 0904:2015
"LibUSB-1.0: Baum [EcoVario 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2015

; Device: 0904:2016
"LibUSB-1.0: Baum [EcoVario 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_2016

; Device: 0904:3000
"LibUSB-1.0: Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3000

; Device: 0904:3001
"LibUSB-1.0: Baum [Orbit in Refreshabraille Emulation Mode (18 cells)], Baum [Refreshabraille 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_3001

; Device: 0904:4004
"LibUSB-1.0: Baum [Pronto! V3 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4004

; Device: 0904:4005
"LibUSB-1.0: Baum [Pronto! V3 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4005

; Device: 0904:4007
"LibUSB-1.0: Baum [Pronto! V4 18 (18 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4007

; Device: 0904:4008
"LibUSB-1.0: Baum [Pronto! V4 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_4008

; Device: 0904:6001
"LibUSB-1.0: Baum [SuperVario2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6001

; Device: 0904:6002
"LibUSB-1.0: Baum [PocketVario2 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6002

; Device: 0904:6003
"LibUSB-1.0: Baum [SuperVario2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6003

; Device: 0904:6004
"LibUSB-1.0: Baum [SuperVario2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6004

; Device: 0904:6005
"LibUSB-1.0: Baum [SuperVario2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6005

; Device: 0904:6006
"LibUSB-1.0: Baum [Brailliant2 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6006

; Device: 0904:6007
"LibUSB-1.0: Baum [Brailliant2 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6007

; Device: 0904:6008
"LibUSB-1.0: Baum [Brailliant2 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6008

; Device: 0904:6009
"LibUSB-1.0: Baum [Brailliant2 64 (64 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6009

; Device: 0904:600A
"LibUSB-1.0: Baum [Brailliant2 80 (80 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_600A

; Device: 0904:6011
"LibUSB-1.0: Baum [VarioConnect 24 (24 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6011

; Device: 0904:6012
"LibUSB-1.0: Baum [VarioConnect 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6012

; Device: 0904:6013
"LibUSB-1.0: Baum [VarioConnect 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6013

; Device: 0904:6101
"LibUSB-1.0: Baum [VarioUltra 20 (20 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6101

; Device: 0904:6102
"LibUSB-1.0: Baum [VarioUltra 40 (40 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6102

; Device: 0904:6103
"LibUSB-1.0: Baum [VarioUltra 32 (32 cells)]"=LIBUSB_DEV, USB\VID_0904&PID_6103

; Device: 0921:1200
"LibUSB-1.0: HandyTech [GoHubs chip]"=LIBUSB_DEV, USB\VID_0921&PID_1200

; Device: 0F4E:0100
"LibUSB-1.0: FreedomScientific [Focus 1]"=LIBUSB_DEV, USB\VID_0F4E&PID_0100

; Device: 0F4E:0111
"LibUSB-1.0: FreedomScientific [PAC Mate]"=LIBUSB_DEV, USB\VID_0F4E&PID_0111

; Device: 0F4E:0112
"LibUSB-1.0: FreedomScientific [Focus 2]"=LIBUSB_DEV, USB\VID_0F4E&PID_0112

; Device: 0F4E:0114
"LibUSB-1.0: FreedomScientific [Focus Blue]"=LIBUSB_DEV, USB\VID_0F4E&PID_0114

; Device: 10C4:EA60
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge / myAVR mySmartUSB light
"LibUSB-1.0: BrailleMemo [Pocket], Seika [Braille Display]"=LIBUSB_DEV, USB\VID_10C4&PID_EA60

; Device: 10C4:EA80
; Generic Identifier
; Vendor: Cygnal Integrated Products, Inc.
; Product: CP210x UART Bridge
"LibUSB-1.0: Seika [Note Taker]"=LIBUSB_DEV, USB\VID_10C4&PID_EA80

; Device: 1148:0301
"LibUSB-1.0: BrailleMemo [Smart]"=LIBUSB_DEV, USB\VID_1148&PID_0301

; Device: 1209:ABC0
"LibUSB-1.0: Inceptor [all models]"=LIBUSB_DEV, USB\VID_1209&PID_ABC0

; Device: 1C71:C004
"LibUSB-1.0: BrailleNote [HumanWare APEX]"=LIBUSB_DEV, USB\VID_1C71&PID_C004

; Device: 1C71:C005
"LibUSB-1.0: HumanWare [all models (serial protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C005

; Device: 1C71:C006
"LibUSB-1.0: HumanWare [non-Touch models (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C006

; Device: 1C71:C00A
"LibUSB-1.0: HumanWare [BrailleNote Touch (HID protocol)]"=LIBUSB_DEV, USB\VID_1C71&PID_C00A

; Device: 1FE4:0003
"LibUSB-1.0: HandyTech [USB-HID adapter]"=LIBUSB_DEV, USB\VID_1FE4&PID_0003

; Device: 1FE4:0044
"LibUSB-1.0: HandyTech [Easy Braille (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0044

; Device: 1FE4:0054
"LibUSB-1.0: HandyTech [Active Braille]"=LIBUSB_DEV, USB\VID_1FE4&PID_0054

; Device: 1FE4:0055
"LibUSB-1.0: HandyTech [Connect Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0055

; Device: 1FE4:0061
"LibUSB-1.0: HandyTech [Actilino]"=LIBUSB_DEV, USB\VID_1FE4&PID_0061

; Device: 1FE4:0064
"LibUSB-1.0: HandyTech [Active Star 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0064

; Device: 1FE4:0074
"LibUSB-1.0: HandyTech [Braille Star 40 (HID)]"=LIBUSB_DEV, USB\VID_1FE4&PID_0074

; Device: 1FE4:0081
"LibUSB-1.0: HandyTech [Basic Braille 16]"=LIBUSB_DEV, USB\VID_1FE4&PID_0081

; Device: 1FE4:0082
"LibUSB-1.0: HandyTech [Basic Braille 20]"=LIBUSB_DEV, USB\VID_1FE4&PID_0082

; Device: 1FE4:0083
"LibUSB-1.0: HandyTech [Basic Braille 32]"=LIBUSB_DEV, USB\VID_1FE4&PID_0083

; Device: 1FE4:0084
"LibUSB-1.0: HandyTech [Basic Braille 40]"=LIBUSB_DEV, USB\VID_1FE4&PID_0084

; Device: 1FE4:0086
"LibUSB-1.0: HandyTech [Basic Braille 64]"=LIBUSB_DEV, USB\VID_1FE4&PID_0086

; Device: 1FE4:0087
"LibUSB-1.0: HandyTech [Basic Braille 80]"=LIBUSB_DEV, USB\VID_1FE4&PID_0087

; Device: 1FE4:008A
"LibUSB-1.0: HandyTech [Basic Braille 48]"=LIBUSB_DEV, USB\VID_1FE4&PID_008A

; Device: 1FE4:008B
"LibUSB-1.0: HandyTech [Basic Braille 160]"=LIBUSB_DEV, USB\VID_1FE4&PID_008B

; Device: 4242:0001
"LibUSB-1.0: Pegasus [all models]"=LIBUSB_DEV, USB\VID_4242&PID_0001

; Device: C251:1122
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1122

; Device: C251:1123
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1123

; Device: C251:1124
"LibUSB-1.0: EuroBraille [Esys (version < 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1124

; Device: C251:1125
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1125

; Device: C251:1126
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, no SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1126

; Device: C251:1127
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1127

; Device: C251:1128
"LibUSB-1.0: EuroBraille [Esys (version >= 3.0, with SD card)]"=LIBUSB_DEV, USB\VID_C251&PID_1128

; Device: C251:1129
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1129

; Device: C251:112A
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112A

; Device: C251:112B
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112B

; Device: C251:112C
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112C

; Device: C251:112D
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112D

; Device: C251:112E
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112E

; Device: C251:112F
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_112F

; Device: C251:1130
"LibUSB-1.0: EuroBraille [Esytime (firmware 1.03, 2014-03-31)], EuroBraille [Esytime]"=LIBUSB_DEV, USB\VID_C251&PID_1130

; Device: C251:1131
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1131

; Device: C251:1132
"LibUSB-1.0: EuroBraille [reserved]"=LIBUSB_DEV, USB\VID_C251&PID_1132

; END_USB_DEVICES

; ==================== Installation ===================

; The Include and Needs directives in the LIBUSB_DEV section are required for 
; installing WinUSB on Windows Vista systems. Windows XP systems ignore these 
; directives. These directives should not be modified.
[LIBUSB_DEV]
Include=winusb.inf
Needs=WINUSB.NT

; The Include directive in the LIBUSB_DEV.Services section includes the system-
; supplied INF for WinUSB. This INF is installed by the WinUSB co-installer if 
; it is not already on the target system. The AddService directive specifies 
; WinUsb.sys as the device�s function driver. These directives should not be 
; modified.
[LIBUSB_DEV.Services]
Include=winusb.inf
AddService=WinUSB,0x00000002,WinUSB_ServiceInstall

; The WinUSB_ServiceInstall section contains the data for installing WinUsb.sys 
; as a service. This section should not be modified.
[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

; The KmdfService directive installs WinUsb.sys as a kernel-mode service. The 
; referenced WinLIBUSB_DEV section specifies the KMDF library version. 
; Usually, the version can be derived from the WdfCoInstallerxxyyy.dll with 
; xx = major, yyy = minor
[LIBUSB_DEV.Wdf]
KmdfService=WINUSB, WinLIBUSB_DEV

[WinLIBUSB_DEV]
KmdfLibraryVersion=1.9

; LIBUSB_DEV.HW is the key section in the INF. It specifies the device 
; interface globally unique identifier (GUID) for your device. The AddReg 
; directive puts the interface GUID in a standard registry value. When 
; WinUsb.sys is loaded as the device�s function driver, it reads the registry
; value and uses the specified GUID to represent the device interface. You 
; should replace the GUID in this example with one that you create specifically
; for your device. If the protocols for the device change, you should create a
; new device interface GUID.
[LIBUSB_DEV.HW]
AddReg=Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,%DeviceGUID%

; The LIBUSB_DEV.CoInstallers section, including the referenced AddReg and 
; CopyFiles sections, contains data and instructions to install the WinUSB and 
; KMDF co installers and associate them with the device. Most USB devices can 
; use these sections and directives without modification.
[LIBUSB_DEV.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01015.dll,WdfCoInstaller","WinUsbCoinstaller3.dll"

[CoInstallers_CopyFiles]
WinUsbCoinstaller3.dll
WdfCoInstaller01015.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

; =============== Source Media Section ================
 
; The x86, x64 and arm64 versions of Windows have separate co installers. This example 
; stores them on the installation disk in separate directories.
[SourceDisksNames]
1 = %DiskName%,,,\i386
2 = %DiskName%,,,\amd64
3 = %DiskName%,,,\arm64

[SourceDisksFiles.x86]
WinUsbCoinstaller3.dll=1
WdfCoInstaller01015.dll=1

[SourceDisksFiles.amd64]
WinUsbCoinstaller3.dll=2
WdfCoInstaller01015.dll=2

[SourceDisksFiles.arm64]
WinUsbCoinstaller3.dll=3
WdfCoInstaller01015.dll=3
